Measurements in Physics

 Laboratory Exploration

**Purpose**:

* To introduce scientific measuring instruments.
* To practice measuring *accurately* with these instruments.
* To achieve mastery in reporting measurements to the correct number of significant digits based on the *precision* of the instruments.

**Materials**:

* Measurement kit containing: Vernier caliper, micrometer, depth gauge, metric ruler, aluminum square, plastic vial, graduated cylinder, steel ball.

**Procedure**:

Inner and outer diameters (a.k.a. internal and external diameters)

1. Measure the outer diameter of the plastic graduated cylinder.
	1. Place the plastic graduated cylinder on the lab table. Hold the cylinder with one hand.
	2. Using the ruler, measure the distance across the top of the cylinder. Record the distance from the outer edge of one side to the outer edge of the opposite side.
	3. Record your measurement correctly in centimeters. Convert your centimeters into millimeters. Remember to record the correct number of significant figures.
	4. Measure the outer diameter with the caliper. Using the ridged lines on the lower part of the Vernier caliper, open up the caliper all the way. Place the caliper over the outside edges of the cylinder.
	5. Carefully slide the sliding scale of the caliper until the lower parallel sides of the caliper touch the cylinder. Observe where the last line on the moveable section of the caliper lies directly under another line. Record your measurement correctly in centimeters. Convert your centimeters into millimeters. Remember to record the correct number of significant figures.
2. Measure the inner diameter of the plastic graduated cylinder.
	1. Place the graduated cylinder on the lab table. Hold it in one of your hands.
	2. Using the ruler, measure the distance across the top of the cylinder from the inner edge of one side to the inner edge of the opposite side.
	3. Record your measurement correctly in centimeters. Convert your centimeters into millimeters. Remember to record the correct number of significant figures.
	4. Measure the inner diameter of the cylinder with the caliper. Invert the caliper so the upper part of the caliper is inserted into the inside of the cylinder. Place your thumb on the ridged section. Slowly move the caliper until the parallel parts for the internal measurement are touching the sides of the cylinder.
	5. Carefully observe the inside bottom of the caliper to take your measurement in centimeters. Observe the last line of the bottom of the moveable part of the caliper to determine the internal measurement of the cylinder.
	6. Convert your centimeters into millimeters. Remember to record the correct number of significant figures.
3. Calculating circumference and volume
	1. Determine the circumference of the cylinder based on the outer diameter obtained from the ruler in centimeters.
	2. Repeat the calculation using the diameter obtained from the caliper in centimeters. Record your answers in the correct number of significant figures.
	3. Determine the depth of the cylinder using the depth gauge accessory on the caliper. Record your answer in centimeters using the correct number of significant figures.
	4. Calculate the total volume of the cylinder in cubic centimeters using the measurements taken with the ruler and with the measurements taken with the caliper and depth gauge. Record your answer with the correct number of significant figures.

Length, Width, Area and Volume

1. Measure the length, width and height.
	1. Obtain the aluminum square. Using the ruler, measure and record the length, width and height of the aluminum square. Record your answer in centimeters using the correct number of significant figures.

length

width

height

* 1. Calculate and record the area of the face of the aluminum square. Calculate and record the volume of the aluminum square. Record all data using the correct number of significant figures.
	2. Measure and record the length, width and height measurements with the caliper. Calculate and record the area of the face of the aluminum square. Calculate and record the volume of the aluminum square. Record all data using the correct number of significant figures.
1. Obtain measurements with a micrometer.
	1. Remove the micrometer from the measurement kit.
	**Your micrometer is a precise instrument and should never be over tightened.** Place the handle of the cylinder in one hand, and with the other hand, hold the rounded bottom. Turn the revolving barrel counterclockwise. Observe the units of measurement on the rounded shaft. Turn the moveable barrel counterclockwise or clockwise until the 0 line is perfectly horizontal to the horizontal line. Note that one turn of the barrel represents one millimeter.
	2. Carefully turn the micrometer in a counterclockwise direction until it is opened wider than the height of the aluminum square. Carefully slide the aluminum square into the micrometer. Turn the barrel clockwise until it is touches the aluminum square. **Turn the knurled knob on the end of the micrometer one “click” to achieve the desired tightness for measurement – remember: do not over tighten.** Record the height of the aluminum square with the correct number of significant figures.
	3. Calculate the area of the face and volume of the square using the caliper length and width measurements and the micrometer height measurement. Record the area and volume using the correct number of significant figures.

Challenge (optional, as time allows):

1. Measure and record the volume of pulp required to manufacture a sheet of notebook paper. Record your measurements and calculations using the correct number of significant figures.

**Sample Data Table (**you may use this one or create your own)**:**

Graduated Cylinder

|  |  |  |
| --- | --- | --- |
| Dimension | Metric ruler | Caliper |
| Outer diameter | 1.5 cm | 1.5 cm |
|  | 15.0 mm | 15.0 mm |
| Inner diameter | 1.3 cm | 1.3 cm |
|  | 13.0 mm | 13.0 mm |
| Circumference | 4.7 cm | 4.7 cm |
| Depth | 10 cm |  10.44 cm |
| Volume | 13.27 cm3 | 13.86 cm3 |

Aluminum Square

|  |  |  |  |
| --- | --- | --- | --- |
| Dimension | Metric Ruler | Caliper | Micrometer |
| length | 2.5 cm | 2.5 cm | 2.512 cm |
| width | 2.55 cm | 2.57 cm | 2.578 cm |
| height | 0.1 cm | 0.15 cm | 0.1532 cm |
| Area | 6.4 cm2 | 6.4 cm2 | 6.476 cm2 |
| Volume | 0.6 cm3 | 0.96 cm3 | 0.9921 cm2 |

**Analysis:**

1. Compare and contrast *accuracy* and *precision*. Consider how one could improve the accuracy of a measurement? the precision of a measurement?

Precision is based on the function of the instrument that you are using. Different instruments, like the micrometer is more precise than others like the metric ruler. Accuracy is based on the person who uses the instrument. Different people will see different measures based on their ability to discern. To improve accuracy, you can take the measurement multiple times. You can also have someone else take the measurement and compare the results. To improve the precision of measurement you can use a toll that is more precise such as the micrometer compared to a ruler.

1. Compare the number of significant figures in the calculations and measurements taken with the ruler to the measurements taken with the caliper and micrometer. Discuss the differences in precision of these instruments.

The metric ruler can only measure up to millimeters. The caliper can measure up to one tenth of a millimeter, while the micrometer can measure up to a micrometer. The micrometer is the most precise of the three instruments because it can measure to the most significant digits. The metric ruler is the least precise because it can only measure to a millimeter.

1. Compare your measurements and calculations with those of a classmate. Are they the same? Discuss sources of error in the *accuracy* of the measurements.

 When I compared my measurements with another classmate I found that our measurements were all very close to one another, differing by little more than a millimeter. The differences between our measurements are based on error in the accuracy of our measurements. The accuracy errors are caused by our personal ability to read the tiny markings on the tools that we were using.

4. Which instrument is more precise, the metric ruler, micrometer or caliper?

 The most precise instrument is the micrometer. It is the most precise because it can measure down to the micrometer, which has more significant figures than the caliper, which measures to the nearest tenth of a millimeter, and the metric ruler, which measures to the nearest millimeter.